{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["工作危害分析表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"工作危害分析表","index":0,"n_rows":4,"n_cols":17,"rows_kept":4,"cut":false,"hidden":false,"merged":[[0,0,0,10],[1,5,1,8],[1,10,1,14],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,15,2,15],[1,16,2,16]]}
["工作危害分析（JHA）评价记录表"]
["风险编号","作业活动","工作步骤","危害因素或潜在事件识别","危害产生的后果","安全风险分析",null,null,null,"安全风险评价","控制措施",{"$nulls":4},"管控层级","管控主体"]
[{"$nulls":5},"可能性（L）","频繁程度（E）","后果严重性（C）","风险度（D）","安全风险等级","工程技术","管理","培训教育","个体防护","应急处置"]
["LS(二)-FX03-2039 ","一二期干吸工段检修","干吸工段现场隔膜压力表","浓酸误接触、二氧化硫三氧化硫气体泄露","化学灼伤、中毒、窒息",{"$nulls":10}," 车间级","用户真实姓名"]