{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["工作危害分析表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"工作危害分析表","index":0,"n_rows":4,"n_cols":16,"rows_kept":4,"cut":false,"hidden":false,"merged":[[0,0,0,15],[1,5,1,8],[1,10,1,14],[1,0,2,0],[1,15,2,15],[1,1,1,4]]}
["风险（LEC）评价表"]
["风险编号","危险源信息",null,null,null,"安全风险分析",null,null,null,"安全风险评价","控制措施",{"$nulls":4},"管控层级"]
[null,"危险源","风险项","危害因素或潜在事件识别","危害产生的后果","可能性（L）","频繁程度（E）","后果严重性（C）","风险度（D）","风险等级","工程技术","管理","培训教育","个体防护","应急处置"]
["DL-FX06-1035","设备","干吸工段现场隔膜压力表","浓酸误接触、二氧化硫三氧化硫气体泄露","化学灼伤、中毒、窒息",{"$nulls":4},"红色",{"$nulls":5}," 车间级"]